FRISBEE GOLF

TARGETS

 **TO MAKE THIS ACTIVITY AT HOME, YOU WILL NEED THE FOLLOWING PARTS:**

**1 - HULA HOOP (pvc tubing – you will make this)**

**1 – ¾ INCH PVC 3 WAY PIPE CONNECTOR (T shape connector)**

**1 – ¾ INCH PVC PIPE CUT TO 5 FOOT LENGTH PER TARGET (or your choice)**

**1 – PLASTIC COFFEE CAN WITH LID PER TARGET (stand/base)**

 **BAGS OF SAND OR CEMENT (amount needed will be based on numbers created)**

**1 – 1 INCH PVC PIPE INSERT (cut to fit- optional part)**

**1 – FLAG/ HOLE NUMBER SIGNAGE (2 cable ties to hold in place)**

**1 – PVC PIPE CUTTER**

**WHAT’S NEXT?**

Purchase PVC piping that is used for underground sprinklers to make the hoop target. They come in rolls of different lengths and sizes at most local hardware stores. **When purchasing your connectors and the PVC pipe for the stand, make** **sure they are all the same size**. I used ¾ inch for this presentation, but you can use 1 inch pipe and fittings that match your pipe size used.

**STEP ONE:** Take the T-Connector and using a rubber mallet, gently tap the T into one of the openings of the 5-ft. long PVC pipe that will serve as the stand for the hoop target. Tap T into pipe until flush with the pipe or close as possible.

**STEP TWO:** Cut the Hulu Hoop to desired size using the pipe cutters. Heat one end of pipe tube using a Hot Gun until the plastic begins to soften (it will look gooey). Insert one end of the T-Connector that is now attached to the 5-ft. stand into that heated opening and slide the plastic tube up to the center mark on the connector. Heat the remaining side in the same manner and slide that tube side to center mark so both ends of tube are touching each other or close as possible. At this point, the hoop and stand are now one piece looking like a large lolly pop!

**STEP THREE:** Fill the coffee can base with either sand or cement to create a sturdy base for the hoop target. Cut a hole that is just a bit larger than the stand on the lid so the stand can pass through the top and thus have support to stand up during play (if using sand, you will need to seal the cut opening of the lid so the sand will not spill out using caulking, expanding foam spray, etc.). One trick to help support the stand is to use the next PVC pipe size up. This will act as an insert to help hold the target. This insert will enter into the base (coffee can) and stick out the top of lid by up to 4 inches. Place tape over the bottom end of this insert tube so it will cover the opening preventing the cement/sand from creating a blockage. By using this combination, it will allow the stand/hoop target to be removed from the base allowing for better storage when not in use. The insert will/can remain in the base (coffee can).

**STEP FOUR:** Set up your golf course for inside or outside play!